[bookmark: _GoBack]New DC Roam Firmware Update (Ver. 0925)
1. Firstly, upgrade the firmware (IocRelease-ssd202-BootUpgradeDC202-dc-20260925-082555.zip), wait 30 seconds and reboot the charger.
2. Upgrade the second firmware (IocRelease-CombinationPackage-Portable202-20260618-191757), wait 1 min and reboot the charger
3. Upgrade the third firmware (IocRelease-CombinationPackage-PortableWeb-20260618-191757.zip), wait 1 min and reboot the charger

Download the log and open the zipfile, and check boot_upgrade_indep.xxxxxxx.log

Ctrl+F quick search ‘upgrade_handle.’ , to see all commands with ,pass.
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4. Upgrade the third firmware (IocRelease-b103-dispenser_103-20260604-190501), wait 3 mins, power-cycle the charger

Download the log and open the zipfile, and check the dispenser_mngr.xxxxx.log.

Ctrl+F quick search ‘swVer’ and you will find swVer 00000000 -> xxxxx, if xxxxx is larger than 20260201, then it proves the firmware update is successful.
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5. Please check the App version, then conduct the test.
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deamon. c:165]@[@mnan

VER x

deamon. c:171]8[@n patcn_r1sTi| arspenser_to3- japom
deamon. :165]8[@mname : dispenser_rf, version:20260618-1917368[0m

deamon.c:171]8[em patch_list:(null)E[em

deamon. c:165]8[@mname: homeOcpp, version:20260618-1917188[0m

deamon. c:171]8[ém patch_list:["net202"]8[om

Charger_DrvBoard_MQTT. c:579]8[@mSuccessfully subscribed to topic: /boot/global/upgrade-info, mid: 4B[om
Charger_DrvBoard_MQTT. c:579]8[@mSuccessfully subscribed to topic: /boot/global/rom-info, mid: SE[0m
Upgrade_handle.c:319]8[@nInstalled module:cabinet_web:20260618-191720, passE[ém
upgrade_handle.c:319]8[@nInstalled module:dispenser_lvgl_1024_600_single:20260618-191756, passE[eém
upgrade_handle.c:319]8[@nInstalled module:dispenser_mngr:20260618-191723, passE[eén
upgrade_handle.c:319]8[@nInstalled module:dispenser_PLC:202606041448, passE[ém
upgrade_handle.c:319]8[@nInstalled module:homeOcpp:20260618-191718, passE[om

upgrade_handle.c:319]8[@nInstalled module:dispenser_meter:20260618-191730, passd[em

upgrade_handle.c:319]8[@nInstalled module:dispenser_rf:20260618-191736, passa[em

deamon. c:615]8[@m[ cabinet_web]:kill: you need to specify whom to kill
17:43: can not find port
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"nodePerContactor™ s

Charger_GBTRNL_Statushingr.c:646]a[enCP @ -> 43[em
Charger_UpperTrans. c:1275]8[@nPresVolt/Curr: © / 0B[om

Charger_Modbus. c:434]8[@mupgCode 00006008 -> 25211516B[0m

Charger_Modbus.c:443]E[@nswVer 00000000 -> 26050901E[0m
Charger_Modbus .c:563]8[@mAux Relay @ -> 18[em

Charger_Modbus. c:535]B[@nCP Voltage(0.1V) @ -> 1218[om

Charger_Modbus. c:612]8[@mInsu RP @ -> 65535B[0m

2 0f7

Charger_Modbus. c:612]B8[@nInsu RP @ ->
Charger_DrvPoint_Stack.c:26]8[@m[645]
Charger_DrvPoint_Stack.c:26]8[@m[645]
Charger_DrvPoint_Stack.c:10]E[@m[709]
Charger_DrvPoint_Stack.c:10]8[@m[715]

Charger_DrvPoint_Stack.c:10]8[@m[952]

characters. Blain text

655358 0m

ConnTemp[@]: @ -> 203[em
ConnTemp[1]: @ -> 193[em
spd[e]: @ -> 15[en
rdcExchk[@]: @ -> 18[em

Temperature[@]: @ -> -1283[6m
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